2-06.5	Measurement and Payment
(March 9, 2016 APWA GSP)

Supplement this section with the following:

Measurement for Subgrade for Permeable Pavement will be in accordance with 2-06.5.