4-04.3(5)	Shaping and Compaction
(March 9, 2016 APWA GSP)

Supplement this section with the following:

Immediately following spreading and final shaping each layer of surfacing shall be lightly compacted in one lift until no visible movement of aggregate is observed resulting in a firm and unyielding condition, as determined by the Engineer.