4-04.4	Measurement
(March 9, 2016 APWA GSP)

Supplement this section with the following:

Crushed Surfacing Choker Course will be measured by the ton in accordance with Section 1-09.2, based on certified truck tickets collected by the Contractor and provided to the inspector at the end of each working day.