5-04.3(8)A6	Test Methods
(March 9, 2016 APWA GSP)

Supplement this section with the following:

The temperature of the mix at the time of discharge from the haul vehicle shall be within the temperature range identified in the approved PHMA submittal.