5-04.3(9)	Spreading and Finishing
(March 9, 2016 APWA GSP)

Supplement this section with the following:

Placement temperature of the mixture shall be within the temperature range identified in the approved PHMA/PWMA submittal.