5-04.4	Measurement
(March 9, 2016 APWA GSP)

Supplement this section with the following:

PHMA/PWMA will be measured by the ton in accordance with Section 1-09.2, with no deduction being made for the weight of asphalt binder, blending sand, mineral filler, or any other component of the HMA. If the Contractor elects to remove and replace mix as allowed in Section 5-04.3(11), the material removed will not be measured.